**Ladson Road**

**Public Right-of-Way Construction Impacts**

**Side:** East

**Limits:** Ordway to Edgewood

**Sidewalk Width:** 5-Ft

**Sidewalk Material:** Concrete

**Road Width:** 23’ (gutter to gutter)

|  |  |
| --- | --- |
| **ADDRESS** | **CONSTRUCTION IMPACTS** |
| **For All Addresses** | Construct a 5’ wide concrete sidewalk adjacent to curb without grass buffer.  Remove a total of 525 LF of curb and replace with barrier curb. |
| **318 Ladson** | Remove and replace brick lead walk with concrete lead walk within public right of way.  Remove and reset existing traffic sign and support. |
| **316 Ladson** | Remove and replace concrete lead walk. |
| **314 Ladson** | Remove and replace concrete lead walk. |
| **312 Ladson** | Remove and replace concrete lead walk. |
| **310 Ladson** | Remove brick lead walk and replace with concrete.  Remove tree with 51” diameter in poor health. New trees may be planted. |
| **308 Ladson** | Remove and replace concrete lead walk. |
| **306 Ladson** | Remove and replace concrete lead walk. |
| **304 Ladson** | Remove and replace concrete driveway apron.  Remove and replace concrete lead walk.  Place sidewalk in front of lamp post. |
| **302 Ladson** | Remove and replace concrete driveway apron.  Remove and replace concrete lead walk.  Shift curb into existing roadway to allow for concrete sidewalk to be installed with back edge aligned with existing back of curb. |
| **10602 Ordway** | Remove tree with 27” diameter in poor health. New trees may be planted.  Construct pedestrian ramp crossing Ordway Drive.  Remove and reset existing traffic signs and support.  Reduce curb radius on corner. |
| **10607 Ordway** | Construct pedestrian ramp crossing Ordway Drive.  Install sign. |

**☞ The above impacts are based on a preliminary investigation and are subject to change at any time as field conditions warrant.**