**Marvin Road**

**Public Right-of-Way Construction Impacts**

**Side:** West

**Limits:** Ordway to Edgewood

**Sidewalk Width:** 5-Ft

**Sidewalk Material:** Concrete

**Road Width:** 23’ (gutter to gutter)

|  |  |
| --- | --- |
| **ADDRESS** | **CONSTRUCTION IMPACTS** |
| **For All Addresses** | Construct a 5’ wide concrete sidewalk with a 2-3’ green space.Remove a total of 525 LF of curb and replace with barrier curb. |
| **315 Marvin**  | Construct pedestrian ramp at corner.Relocate existing traffic signs.Remove and replace concrete lead walk and steps within public right of way.Construct a retaining wall or backer curb as needed to tie into existing grade.Place sidewalk behind pole #795435-2503.Adjust storm drain top. |
| **313 Marvin** | Remove and replace concrete lead walk.Construct a retaining wall or backer curb as needed to tie into existing grade.Place sidewalk behind pole #795435-290140. |
| **311 Marvin**  | Remove and replace concrete lead walk.Remove and replace concrete driveway apron.Adjust water valve and gas valve covers. |
| **309 Marvin** | Remove brick lead walk and replace with concrete.Trim tree branches.Place sidewalk behind pole #795435-360240.Relocate utility guy wire, as needed. |
| **307 Marvin** | Remove brick lead walk and replace with concrete.Remove tree with 21” diameter. A new tree may be planted. |
| **305 Marvin** | Remove HMA apron and replace with concrete driveway apron.Place sidewalk behind fire hydrant.Place sidewalk behind pole #795435-460320.Remove and replace concrete lead walk within public right of way. |
| **303 Marvin**  | Remove and replace concrete driveway apron.Remove and replace concrete lead walk. |
| **10600 Ordway** | Place sidewalk behind pole #795435-570400 and move anchors.Construct an ADA ramp.Construct a retaining wall or backer curb as needed to tie into existing grade. |

**☞ The above impacts are based on a preliminary investigation and are subject to change at any time as field conditions warrant.**